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e CST 2-187, (315) 443-3948 s
%
wec<int> myVec(5): /7 create vector with 5 elements
int val nyVec[3] 7 /7 read/write to 4th element
int len = myVec.size(): /7 read myVec's size
nyVec.size(7); /7 change nyVec's size, keep elements
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