CPU status flags (The EFLAGS register contents)

	Flag 
	VS.NET

Mnemonic
	Intel

Mnemonic
	Notes

	Overflow
	OV
	OF
	 

	Direction
	UP
	DF
	Indicates the direction of string processing. 1 means highest address to lowest. 0 means lowest address to highest address

	Interrupt

Enable
	EI
	IF
	Set to 1 if interrupts are enabled. This is always set to 1 by a user mode debugger

	Sign 
	PL
	SF
	 

	Zero
	ZR
	ZF
	 

	Auxiliary Carry
	AC
	AF
	Indicates a carry/borrow in BCD arithmetic

	Parity
	PE
	PF
	 

	Carry
	CY
	CF
	 


