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Out of Process Component Diagrams
Purpose:
Illustrate the structure and operation of out-of-process COM components.  These come in two flavors:

1. Single Threaded Apartment (STA) components:
Client messages are marshaled through an STA channel that uses a windows message loop to serialize access to the component for concurrent clients.  The server is held in memory by servicing the message loop.

2. Multi-Threaded Apartment (MTA) components:
Client messages are marshaled through an MTA channel that dispatches RPC threads without channel synchronization.  This means that the designer must synchronize all shared data.  The server is held in memory by blocking on an event.
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