	Module
	RI
	Issue
	B-Spec Req #
	Necessitates non-delivery of TP
	Text

	UI
	Abhishek
	Delegation requirement is hard to be tested
	3.2.1.1.3.2g
	Y
	It shall delegate all operations like saving/retrieving/executing scripts to the Scripting module

	Reporting
	Abhishek
	Delegation requirement is hard to be tested
	3.2.1.1.1.2j
	Y
	It shall delegate all file transfer operations like copy/match/rollback to the FileTransfer module.

	Reporting
	Abhishek
	Reporting don’t assign Operation numbers
	3.2.1.1.1.2i
	Y
	It shall provide an operation number for each operation. Operation number is a sequence number for user request. For example, when user clicks the copy control, this process needs to generate a sequence number for this copy request.

	Reporting
	Abhishek
	Reporting don’t assign Operation numbers
	3.2.1.1.2.2j
	Y
	It shall provide an operation number for each operation. Operation number is a sequence number for user request. For example, when user clicks the copy control, this process needs to generate a sequence number for this copy request.

	Reporting
	Abhishek
	Delegation requirement is hard to be tested
	3.2.1.1.2.2k
	Y
	It shall delegate all registry operations for copy/match/backup/rollback to the Registry module.

	Script
	Jeff
	4.2.1.4.2.a(3.2.1.3) -- add to the process reqs section fo script, do a code wlakthrought to test
	 
	 
	It shall send each incoming  script command to its respective module (File Transfer or Registry) in the format requested by the receiving module for execution without user interaction.

	Registry
	Mithun
	To be removed - Valid .reg
	5.2.1.1.2.l (Last shall)
	Backup – restore operation.
	During qualification test a valid .reg file shall  be exported and used as a test registry pattern.

	Registry
	Mithun
	Rollback file format changed to .rbk
	5.2.1.2.2.c
	Changed to .rbk file
	Rollback information shall be saved in a .reg file for registry transfers.

	Registry
	Mithun
	Test stubs - 1 COM Library - Cannot have test stub
	 
	 Use test driver now.
	Every module shall have functional test-stubs that exercise the complete functionality of that module.

	Comm
	Sashi
	modify b-spec to remove "connection received" notification
	6.2.1.1.2.e
	RD,KG to reword
	shall send out notification message in case of any new connection received and any new connection established

	Comm
	Sashi
	current communication architecture follows a connect - transfer - disconnect protocol.
	6.2.1.2.2.2.c
	 Copy/match operation – by analysis.
	This process shall send a connection request over network to remote machine with given IP address in order to establish a connection

	Comm
	Sashi
	code not connection oriented.
	6.2.1.2.3.2.d
	 RD,KG to reword
	

	Comm
	Sashi
	code not connection oriented.
	6.2.1.2.3.2.e
	 RD,KG to reword
	This process shall generate status messages regarding status of connection



	Comm
	Sashi
	issues regarding IP validation and connection established message.
	6.2.1.2.1.2.a,b,c
	 Takeall  OFF the B-Spec .
	· shall validate the machine IP address

· shall give out an error message if the IP address is not valid

· If the connection is already established, shall give a message indicating that the connection is made



	 Scripting
	 Jeff
	 Issues regarding how to test script delegation
	 4.2.1.1.2.a
	 
	This process shall delegate tasks through its sub-processes to the Reporting, File Transfer and Registry module depending upon the user commands.

	 Scripting 
	Jeff
	 Issues regarding how to map the A-spec 3.1.9
	 To be added 
	 
	It shall be able to execute all the file transfer or registry transfer operations except rollback operations through file transfer module or registry module

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	

	 
	 
	 
	 
	 
	


