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Server_Test 3 – To show that when the client receives an error indication saying file or manifest transfer failed, client shall send an error message to the user.

Requirements:

Interface_9:

Upon receipt of an error indication that the file or manifest transfer failed, the Foundry client shall send an error indication to the user

Test Description:

In this test, the server is up and running, and a client on the remote machine is connected to it. The server will start sending a file, which will be pre-stored on a defined location on its hard drive. Half way through the transfer, the cable connecting the PC to the network is removed. This will signify that the transfer is not complete and the client will display an error message to the user stating the same.

Pre-Conditions:

1. File transfer.cs is available on a <basedir>\Client\Client2\Other.

2. Carry on from Server_Test 1

Test Procedures – Demonstration:

a. In the client form on remote machine, go to the upload file section and click on browse.

b. When browse window pops up, choose <basedir>\Client\Client2\Other \transfer.cs and click open.

c. Click “OK” on the client forms “upload file” section.

d. Immediately after clicking “OK” yank out the network connection cable from the CPU. (Note: One must give the system practical time for the transfer to begin, but not complete. The file is 10.6 MB in size, hence it takes time to upload!)

e. Client will show on its interface a message which says, “An Existing Connection was forcibly closed by remote host”

(Satisfies Interface_9)
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